|  |
| --- |
|  |

|  |  |
| --- | --- |
| **Plastic Grain Mixer (Big Mixer)** | |
| **INNER DIAMETER** | 1500mm\*560mm |
| **CAPACITY** | 500kg |
| **MACHINE SIZE** | 1.7m\*1.58\*1.5 |
| **MACHINE WEIGHT** | 500Kg |
| **MODEL/TYPE** | B-15 |
| **MAX OUTPUT** | N/A |
| **VOLTAGE/POWER** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-37Kg -6.3A -EFF: 87.7%**  **-3.0Kw -1410 r/min**  **-380V -50Hz** |
| **MAIN MOTOR SERIAL NO.** | N/A |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | RUIAN QUEENSENSE MACHINE CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **Plastic Grain Mixer (Small Mixer)** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **VOLTAGE/POWER** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-BRAND: DECHANG MOTOR FACTORY**  **-4 Kw -220 V -15.1A -TYPE: YE2-112M-4**  **-1740 r/min -60 Hz -49 Kg -DATE: 2019.12** |
| **MAIN MOTOR SERIAL NO.** | 9061 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | RUIAN QUEENSENSE MACHINE CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **WLCPJ SERIES- AUTOMATIC PLASTIC EXTRUSION BLOW MOLDING MACHINE (GALLON MACHINE #1)** | |
| **MODEL/TYPE** | WLCPJ75IPS |
| **MAX CAPACITY OF PRODUCTION** | 5 L |
| **SCREW DIAMETER** | 75 mm |
| **MOTOR POWER** | 30 Kw |
| **EXECUTIVE STANDARD** | JB/T8539-1997 |
| **SERIAL NO.** | WL20592 |
| **MFG DATE** | 2020-10 |
| **MAX OUTPUT** | N/A |
| **MAIN MOTOR SPECS.** | **-BRAND:** LUAN JIANGHUAI MOTOR CO, LTD.  **-TYPE:** YE2-200L-4 **-STANDARD NO.:** Q/LAE2001-2015  **-POWER:** 30 Kw **-VOLTAGE:** 220 V **-FREQ:** 60 Hz  **-SPEED:** 1776 r/min **-CURRENT:** 99.7 A **-EFF:** 93%  **-WEIGHT:** 227 Kg **-MANUF DATE:** 16.6 |
| **MAIN MOTOR SERIAL NO.** | 697 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **CPJ SERIES- AUTOMATIC PLASTIC EXTRUSION BLOW MOLDING MACHINE**  **(PEANUT BUTTER JAR MACHINE #1)** | |
| **MODEL/TYPE** | CPJ65 II |
| **MAX CAPACITY OF PRODUCTION** | 1X2 L |
| **SCREW DIAMETER** | 65 mm |
| **MOTOR POWER** | 18.5 Kw |
| **EXECUTIVE STANDARD** | JB/T8539-1997 |
| **SERIAL NO.** | WL 18547 |
| **MFG DATE** | 2019-1 |
| **MAX OUTPUT** | N/A |
| **MAIN MOTOR SPECS.** | **-BRAND:** MEIHO  **-MODEL:** Y180M-4 **- HP:** 25  **-POWER:** 18.5 Kw **-VOLTAGE:** 220/440 V **-FREQ:** 60 Hz  **-RPM:** 1760 r/min **-CURRENT:** 62.0/31.9 A |
| **MAIN MOTOR SERIAL NO.** | 17090893 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **WLCPJ SERIES- AUTOMATIC PLASTIC EXTRUSION BLOW MOLDING MACHINE**  **(PEANUT BUTTER JAR MACHINE #2)** | |
| **MODEL/TYPE** | WLCPJ65 II |
| **MAX CAPACITY OF PRODUCTION** | 2X1.0 L |
| **SCREW DIAMETER** | 65 mm |
| **MOTOR POWER** | 18.5 Kw |
| **EXECUTIVE STANDARD** | JB/T8539-1997 |
| **SERIAL NO.** | WL20582 |
| **MFG DATE** | 2020-7 |
| **MAX OUTPUT** | N/A |
| **MAIN MOTOR SPECS.** | **-BRAND:** LUAN JIANGHUAI MOTOR CO, LTD.  **-TYPE:** YE2180M-4 **-STANDARD NO.:** Q/LAE2001-2015  **-POWER:** 18.5 Kw **-VOLTAGE:** 220 V **-FREQ:** 60 Hz  **-SPEED:** 1760 r/min **-CURRENT:** 60 A **-EFF:** 92.3%  **-WEIGHT:** 167 Kg **-MANUF DATE:** 2019.19 |
| **MAIN MOTOR SERIAL NO.** | 1827 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **WLCPJ SERIES- AUTOMATIC PLASTIC EXTRUSION BLOW MOLDING MACHINE**  **(PEANUT BUTTER JAR MACHINE #3)** | |
| **MODEL/TYPE** | WLCPJ65 II |
| **MAX CAPACITY OF PRODUCTION** | (120mm) 2X1.0 L |
| **SCREW DIAMETER** | 65 mm |
| **MOTOR POWER** | 18.5 Kw |
| **EXECUTIVE STANDARD** | JB/T8539-1997 |
| **SERIAL NO.** | WL20617 |
| **MFG DATE** | 2020-12 |
| **MAIN MOTOR SPECS.** | **-BRAND:** GUANGDONG DONGGUAN ELECTRIC MOTOR CO, LTD.  **-TYPE:** YE2-180M-4 **-STANDARD NO.:** JT/T11707  **-POWER:** 18.5 Kw **-VOLTAGE:** 220 V **-FREQ:** 60 Hz  **-SPEED:** 1765 r/min **-CURRENT:** 62.6 A **-EFF:** 91.2%  **-WEIGHT:** 160 Kg **-MANUF DATE:** 2020 10 |
| **MAIN MOTOR SERIAL NO.** | 201001 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **AUTOMATIC PLASTIC EXTRUSION BLOW MOLDING MACHINE (M7)** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-BRAND:** GUANGDONG DONGGUAN ELECTRIC MOTOR CO, LTD.  **-TYPE:** YE2 225S-4 **-STANDARD NO.:** JT/T11707  **-POWER:** 37 Kw **-VOLTAGE:** 220 V **-FREQ:** 60 Hz  **-SPEED:** 1775 r/min **-CURRENT:** 122 A **-EFF:** 92.7%  **-WEIGHT:** 293 Kg **-MANUF DATE:** 2020.06 |
| **MAIN MOTOR SERIAL NO.** | 200602 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **SCJ PLASTIC MOULDING EXPRUSION MACHINE (STRAW MACHINE #1)** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-TYPE:** YX3-80M1-4 **-STANDARD NO.:** GB/T22722-2008  **-POWER:** 0.55Kw **-VOLTAGE:** 380 V **-FREQ:** 50 Hz  **-SPEED:** 1400 r/min **-CURRENT:** 1.57 A **-EFF:** 71%  **-WEIGHT:** 16 Kg **-MANUF DATE:** 2014. 12 |
| **MAIN MOTOR SERIAL NO.** | DL02039 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WEILI PLASTIC MACHINE FACTORY CO., LTD. THE PEOPLES REPUBLIC OF CHINA |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **SCJ PLASTIC MOULDING EXPRUSION MACHINE (STRAW MACHINE #2)** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-TYPE:** YX3-80M2-4 **-STANDARD NO.:** JB/T 10686-2006, GB 18613-2012  **-POWER:** 0.75Kw **-VOLTAGE:** 220 V **-FREQ:** 50 Hz  **-SPEED:** 1400 r/min **-CURRENT:** 3.3 A **-EFF:** 79.6%  **-WEIGHT:** 17 Kg **-MANUF DATE:** 2020. 03 |
| **MAIN MOTOR SERIAL NO.** | 2JC26350 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WEILI PLASTIC MACHINE FACTORY CO., LTD. THE PEOPLES REPUBLIC OF CHINA |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **RECIPROCATING AIR COMPRESSOR (COMPRESSOR #1)** | |
| **POWER** | 15 KW |
| **MOMINAL CAPACITY** | 1.6 M³/min |
| **DISCHAIRCE PRESSURE** | 1.0 Mpa |
| **COMPRESSORSPEED** | 840 r/min |
| **WEIGHT** | 360 Kg |
| **PRODUCTION DATE** | 20 YY – 9 MM |
| **MODEL/TYPE** | W-1.6/10 |
| **Machine Serial No.** | 181 |
| **MAIN MOTOR SPECS.** | **-MANUFACTURED: JIANGSU JIN GU ELECTRIC MACHINERY CO., LTD.**  **-HGHEFFICIENCYTHREE- PHASEASYNCHRONOUSMOTOR**  **-TYPE: YE2-160L-4 -STANDARD: JB/T11707-2013**  **-POWER: 15KW -CURRENT: 50A**  **-VOLTAGE: 220V -PROTECTIONGRADE: IP55**  **-FREQUENCY: 60HZ -EFFICIENCY: 90.6 %**  **-SPEED: 1460/min -MFD: 2020.07** |
| **MAIN MOTOR SERIAL NO.** | N/A |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | (SHANGXING) TAIZHOU HUANGYAN SHANGXING ELECTROME CHANICAL CO., LTD. |
| **LOCATION** | Building #3 Compressor Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **RECIPROCATING AIR COMPRESSOR (COMPRESSOR #2)** | |
| **POWER** | 15 KW |
| **MOMINAL CAPACITY** | 1.6 M³/min |
| **DISCHAIRCE PRESSURE** | 1.0 Mpa |
| **COMPRESSORSPEED** | 840 r/min |
| **WEIGHT** | 350 Kg |
| **PRODUCTION DATE** | 20 YY – 9 MM |
| **MODEL/TYPE** | W-1.6/10 |
| **Machine Serial No.** | 182 |
| **MAIN MOTOR SPECS.** | **-MANUFACTURED: JIANGSU JIN GU ELECTRIC MACHINERY CO., LTD.**  **-HGHEFFICIENCYTHREE- PHASEASYNCHRONOUSMOTOR**  **-TYPE: YE2-160L-4 -STANDARD: JB/T11707-2013**  **-POWER: 15KW -CURRENT: 50A**  **-VOLTAGE: 220V -PROTECTIONGRADE: IP55**  **-FREQUENCY: 60HZ -EFFICIENCY: 90.6 %**  **-SPEED: 1460/min -MFD: 2020.07** |
| **MAIN MOTOR SERIAL NO.** | N/A |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | (SHANGXING) TAIZHOU HUANGYAN SHANGXING ELECTROME CHANICAL CO., LTD. |
| **LOCATION** | Building #3 Compressor Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **HYDRAULLIC CAPS MACHINE** | |
| **MAX. FORMING AREA** | 680 X 300 mm |
| **MAX.HEATING POWER** | 97 Kw |
| **MAX.AIR PRESSURE** | 0.8 Mpa |
| **ASSEMBLING SET WEIGHT** | 4 ton |
| **MAX.FORMING DEPTH** | < 140 mm |
| **MAIN HYDRAULIC PRESSURE** | 80 Mpa |
| **APPLICATION** | PP.HIP.S.PE |
| **DATE OF PRODUCE** | 2019YY 12MM |
| **MODEL/TYPE** | YZC 680 |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | YC-394# |
| **MAIN MOTOR SPECS.** | -**MOTOR POWER**: 7.5 Kw |
| **MAIN MOTOR SERIAL NO.** | N/A |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU MINGFA MACHINERY CO., LTD |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **PLASTIC SHEET MAKING MACHINE** | |
| **SHEET THICKNESS** | 0.4-1.5 mm |
| **L\D RATIO OF SCREW** | 33:1 |
| **MAX OUTPUT** | < 200K/h |
| **EXTERIOR DIMENSION** | 11 X 3.0 X 2.5 m |
| **SHEET WIDTH** | < 720 mm |
| **SCREW DIAMETER** | 100 mm |
| **MAIN MOTOR POWER** | 55 Kw |
| **ASSEMBLING SET POWER** | = 112 Kw |
| **ASSEMBLING WEIGHT** | 10 ton |
| **DATE OF PRODUCE** | 2019 YY 12 MM |
| **MODEL/TYPE** | SLP-100-900 |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | SP-279# |
| **MAIN MOTOR SPECS.** | **-MANUFACTURED: SIEMENS STANDARD MOTORS LTD.**  **-:1TL001-2DBD0 -: IMB3**  **-:9-0AA4-Z -: LMH-1911/800020761812/011**  **-:280S -: Q/321081 KJA002-2018.**  **-: 220 V/380 VY -: 75 Kw**  **-: 60 Hz -: 1782 r/min**  **-: 240/139 A -: COS 0.87**  **-: EFF. 94.5 % -: Th.CL 155 (F)**  **-: IP 55 -: 480 Kg** |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU MINGFA MACHINERY CO., LTD |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **CUTTER MACHINE # 6** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | N/A |
| **MAIN MOTOR SERIAL NO.** | N/A |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | (RUI XING)  Nan’an Ruixing Mechanancial and Electrical Epuiqment LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **AIR RECEIVER (PRINTING COMPRESSOR)** | |
| **MAX. WORKING PRESSURE** | 9 kg/cm² (0.8825985 Mpa) |
| **WATER-TEST PRESSURE** | 14.7 kg/cm² (1.372931 Mpa) |
| **CAPACITY** | 300 l |
| **INSPECTION NO.** | 19180805 |
| **MANUFACTURE DATE** | 07 2019 |
| **MODEL/TYPE** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-MANUFACTURED: HITACHI INDUSTRIAL TECHNOLOGY (THIALAND), LTD.**  **-BRAD: SWAN (THREE PHASE INDUCTION) -10HP -4POLE**  **-MODEL: TFO-KK (TFOD-132M)-4P -WEIGHT: 50 Kg**  **-VOLTS: 220 380 415 220 380 415 -STANDARD EN: 60034-1**  **-HERTZ: 50 50 50 60 60 60 -AMB. TEMP.: 40 °C**  **-AMP’S: 25.8,14.9,14.5,24.7,14.4,13.3**  **-RMP: 1450 1450 1460 1750 1750 1760** |
| **MAIN MOTOR SERIAL NO.** | 19040143 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | TONG CHENG IRON WORKS CO., LTD. |
| **LOCATION** | Building #2 Compressor Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **FLEXOGRAPHIC PRINTING MACHINE** | |
| **MODEL/TYPE** | N/A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | **-MANUFACTURED: HENGLIE**  **-TYPE: YE2-100L1-4 -STANDARD: GB/T28575-2012 -: 34Kg**  **-POWER: 2.2 KW -CURRENT: 4.8 A**  **-VOLTAGE: 380V -PROTECTIONGRADE: IP55**  **-FREQUENCY: 50HZ -EFFICIENCY: 86.7 %**  **-SPEED: 1410/min -MFD: 2021.04** |
| **MAIN MOTOR SERIAL NO.** | 03046 |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | SHANTOU WALEY PLASTIC MACHINERY FACTORY CO., LTD. |
| **LOCATION** | Building #3 Area |

|  |
| --- |
|  |

|  |  |
| --- | --- |
| **BOTTLE PRINTING** | |
| **MODEL/TYPE** | 300-A |
| **MAX OUTPUT** | N/A |
| **Machine Serial No.** | N/A |
| **MAIN MOTOR SPECS.** | N/A |
| **MAIN MOTOR SERIAL NO.** | **-EI – 66X32 -50H2**  **-50VA -8V IIV**  **-220 V** |
| **DATE OF ARRIVAL** |  |
| **DATE OF START UP** |  |
| **MANUFACTURED BY** | N/A |
| **LOCATION** | Building #3 Area |